Chicago Pneumatic CPS90KD Towable Air Compressor

SPECIFICATIONS

88 cfm at 100 psi

Water-cooled 24 hp interim Tier IV Kubota D1105 engine

Heavy-duty 13-in. tires

Folding drawbar

8.5 gal. (32 L) fuel capacity

1,225 lbs. (555 kg)

FEATURES

Easy-to-use centralized Controls

Durable Galvanneal steel enclosure

Powder-coated finish

Torsion bar suspension

Single point lifting bale

Removable side panels

Wide-opening, one-piece hinged hood canopy